;*******************************************************************************
; Copyright 2000, 2001 Altima Corporation.
;
; INF for Windows 2000 , Win Me , and Win 98 SE 
;  
;   Note:   Windows XP (32bit and 64bit) and Windows95 have their
;           own seperate install inf and binaries.
;
; History:
;    06/02/00 Hav Khauv        Inception.
;*******************************************************************************


[Version]
signature="$CHICAGO$"
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
;;CatalogFile=a1kw2k.cat
Compatible= 1
Provider= %ALTM%
DriverVer= 03/26/2002,3.12.0.0

[Manufacturer]
%ALTM% = Altima


[ControlFlags]
;ExcludeFromSelect = *


[Altima]
%ALTIMA1000C%                    = Altima1000C,           PCI\VEN_173B&DEV_03E8&SUBSYS_03E8173B

%ALTIMA1001C%                    = Altima1001C,           PCI\VEN_173B&DEV_03E9&SUBSYS_0001173B

%ALTIMA1002C%                    = Altima1002C,           PCI\VEN_173B&DEV_03EA&SUBSYS_0001173B

%ALTIMA1003C%                    = Altima1003C,           PCI\VEN_173B&DEV_03EB&SUBSYS_0001173B

%ALTIMA1000F%                    = Altima1000F,           PCI\VEN_173B&DEV_03E8&SUBSYS_0003173B

%ALTIMA1000C%                    = Altima1000C,           PCI\VEN_173B&DEV_03E8
%ALTIMA1001C%                    = Altima1001C,           PCI\VEN_173B&DEV_03E9
%ALTIMA1002C%                    = Altima1002C,           PCI\VEN_173B&DEV_03EA
%ALTIMA1003C%                    = Altima1003C,           PCI\VEN_173B&DEV_03EB

;*******************************************************************************
; Win2000 Install sections.
;*******************************************************************************

[Altima1000C.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
AddReg          = Altima.AddReg, Altima.Params
CopyFiles       = CopyFile.Altima.Sys
BusType         = 5

[Altima1000C.NT.Services]
AddService = a1kw2k, 2, Altima1000C.AddService, Altima.EventLog

[Altima1000C.AddService]
DisplayName    = %ALTIMA1000C%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\a1kw2k.sys
LoadOrderGroup = NDIS
AddReg         = Altima.TextModeFlagsReg


[Altima1001C.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
AddReg          = Altima.AddReg, Altima.Params
CopyFiles       = CopyFile.Altima.Sys
BusType         = 5

[Altima1001C.NT.Services]
AddService = a1kw2k, 2, Altima1001C.AddService, Altima.EventLog

[Altima1001C.AddService]
DisplayName    = %ALTIMA1001C%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\a1kw2k.sys
LoadOrderGroup = NDIS
AddReg         = Altima.TextModeFlagsReg


[Altima1002C.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
AddReg          = Altima.AddRegSmall, Altima.Params
CopyFiles       = CopyFile.Altima.Sys
BusType         = 5

[Altima1002C.NT.Services]
AddService = a1kw2k, 2, Altima1002C.AddService, Altima.EventLog

[Altima1002C.AddService]
DisplayName    = %ALTIMA1002C%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\a1kw2k.sys
LoadOrderGroup = NDIS
AddReg         = Altima.TextModeFlagsReg



[Altima1003C.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
AddReg          = Altima.AddReg, Altima.Params
CopyFiles       = CopyFile.Altima.Sys
BusType         = 5

[Altima1003C.NT.Services]
AddService = a1kw2k, 2, Altima1003C.AddService, Altima.EventLog

[Altima1003C.AddService]
DisplayName    = %ALTIMA1003C%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\a1kw2k.sys
LoadOrderGroup = NDIS
AddReg         = Altima.TextModeFlagsReg




[Altima1000F.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
AddReg          = Altima.AddReg, Altima.Fibre.Params
CopyFiles       = CopyFile.Altima.Sys
BusType         = 5

[Altima1000F.NT.Services]
AddService = a1kw2k, 2, Altima1000F.AddService, Altima.EventLog

[Altima1000F.AddService]
DisplayName    = %ALTIMA1000F%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\a1kw2k.sys
LoadOrderGroup = NDIS
AddReg         = Altima.TextModeFlagsReg



; The following is referred by WIN2000 sections above
[Altima.AddReg]
HKR, Ndi,            Service,    0, "a1kw2k"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"

; Altima 100x   4K Jumbo Packet Selection
HKR, Ndi\Params\RxMtu,            ParamDesc, , "Jumbo Mtu"
HKR, Ndi\Params\RxMtu,            default,   , "1500"
HKR, Ndi\Params\RxMtu,            type,      , "dword"
HKR, Ndi\Params\RxMtu,            min,       , "1500"
HKR, Ndi\Params\RxMtu,            max,       , "4000"
HKR, Ndi\Params\RxMtu,            step,      , "500"
HKR, Ndi\Params\RxMtu,            base,      , "10"


[Altima.AddRegSmall]
HKR, Ndi,            Service,    0, "a1kw2k"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"

; Altima 100x   4K Jumbo Packet Selection
HKR, Ndi\Params\RxMtu,            ParamDesc, , "Jumbo Mtu"
HKR, Ndi\Params\RxMtu,            default,   , "1500"
HKR, Ndi\Params\RxMtu,            type,      , "dword"
HKR, Ndi\Params\RxMtu,            min,       , "1500"
HKR, Ndi\Params\RxMtu,            max,       , "1500"
HKR, Ndi\Params\RxMtu,            step,      , "500"
HKR, Ndi\Params\RxMtu,            base,      , "10"


[Altima.EventLog]
AddReg = Altima.AddEventLogReg

[Altima.AddEventLogReg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll;%%SystemRoot%%\System32\drivers\a1kw2k.sys"
HKR, , TypesSupported  , 0x00010001, 7

[Altima.TextModeFlagsReg]
HKR, , TextModeFlags, 0x00010001, 0x0001


;*******************************************************************************
; Win 9x Install sections.
;*******************************************************************************
[Altima1000C]
AddReg    = Altima1000C.W9xAddReg, Altima.W9xAddReg2, Altima.Params
CopyFiles = CopyFile.W9xSys

[Altima1000C.W9xAddReg]
HKR, Ndi, DeviceID,              0, "PCI\VEN_173B&DEV_03E8"
HKR, Ndi\Install,    ndis3,       , "Altima1000C"

; Altima 100x   4K Jumbo Packet Selection
HKR, Ndi\Params\RxMtu,            ParamDesc, , "Jumbo Mtu"
HKR, Ndi\Params\RxMtu,            default,   , "1500"
HKR, Ndi\Params\RxMtu,            type,      , "dword"
HKR, Ndi\Params\RxMtu,            min,       , "1500"
HKR, Ndi\Params\RxMtu,            max,       , "4000"
HKR, Ndi\Params\RxMtu,            step,      , "500"
HKR, Ndi\Params\RxMtu,            base,      , "10"


[Altima1001C]
AddReg    = Altima1001C.W9xAddReg, Altima.W9xAddReg2, Altima.Params
CopyFiles = CopyFile.W9xSys

[Altima1001C.W9xAddReg]
HKR, Ndi, DeviceID,              0, "PCI\VEN_173B&DEV_03E9"
HKR, Ndi\Install,    ndis3,       , "Altima1001C"

; Altima 100x   4K Jumbo Packet Selection
HKR, Ndi\Params\RxMtu,            ParamDesc, , "Jumbo Mtu"
HKR, Ndi\Params\RxMtu,            default,   , "1500"
HKR, Ndi\Params\RxMtu,            type,      , "dword"
HKR, Ndi\Params\RxMtu,            min,       , "1500"
HKR, Ndi\Params\RxMtu,            max,       , "4000"
HKR, Ndi\Params\RxMtu,            step,      , "500"
HKR, Ndi\Params\RxMtu,            base,      , "10"


[Altima1002C]
AddReg    = Altima1002C.W9xAddReg, Altima.W9xAddReg2, Altima.Params
CopyFiles = CopyFile.W9xSys

[Altima1002C.W9xAddReg]
HKR, Ndi, DeviceID,              0, "PCI\VEN_173B&DEV_03EA"
HKR, Ndi\Install,    ndis3,       , "Altima1002C"

; Altima 100x   4K Jumbo Packet Selection
HKR, Ndi\Params\RxMtu,            ParamDesc, , "Jumbo Mtu"
HKR, Ndi\Params\RxMtu,            default,   , "1500"
HKR, Ndi\Params\RxMtu,            type,      , "dword"
HKR, Ndi\Params\RxMtu,            min,       , "1500"
HKR, Ndi\Params\RxMtu,            max,       , "1500"
HKR, Ndi\Params\RxMtu,            step,      , "500"
HKR, Ndi\Params\RxMtu,            base,      , "10"


[Altima1003C]
AddReg    = Altima1003C.W9xAddReg, Altima.W9xAddReg2, Altima.Params
CopyFiles = CopyFile.W9xSys

[Altima1003C.W9xAddReg]
HKR, Ndi, DeviceID,              0, "PCI\VEN_173B&DEV_03EB"
HKR, Ndi\Install,    ndis3,       , "Altima1003C"

; Altima 100x   4K Jumbo Packet Selection
HKR, Ndi\Params\RxMtu,            ParamDesc, , "Jumbo Mtu"
HKR, Ndi\Params\RxMtu,            default,   , "1500"
HKR, Ndi\Params\RxMtu,            type,      , "dword"
HKR, Ndi\Params\RxMtu,            min,       , "1500"
HKR, Ndi\Params\RxMtu,            max,       , "4000"
HKR, Ndi\Params\RxMtu,            step,      , "500"
HKR, Ndi\Params\RxMtu,            base,      , "10"


[Altima1000F]
AddReg    = Altima1000F.W9xAddReg, Altima.W9xAddReg2, Altima.Fibre.Params
CopyFiles = CopyFile.W9xSys


[Altima1000F.W9xAddReg]
HKR, Ndi, DeviceID,              0, "PCI\VEN_173B&DEV_03E8"
HKR, Ndi\Install,    ndis3,       , "Altima1000F"

; Altima 100x   4K Jumbo Packet Selection
HKR, Ndi\Params\RxMtu,            ParamDesc, , "Jumbo Mtu"
HKR, Ndi\Params\RxMtu,            default,   , "1500"
HKR, Ndi\Params\RxMtu,            type,      , "dword"
HKR, Ndi\Params\RxMtu,            min,       , "1500"
HKR, Ndi\Params\RxMtu,            max,       , "4000"
HKR, Ndi\Params\RxMtu,            step,      , "500"
HKR, Ndi\Params\RxMtu,            base,      , "10"



; Common Section Used by W9x Install sections
[Altima.W9xAddReg2]
HKR,    , DevLoader,             0, *ndis
HKR,    , DeviceVxDs,            0, a1kw2k.sys
HKR, , NoEventLogging,             0, "1"

;Windows 95 does not support Ndis5 upper range.
HKR, Ndi\Interfaces, DefUpper,   0, "ndis3"
HKR, Ndi\Interfaces, DefLower,   0, "ethernet"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis3"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"

HKR, NDIS, LogDriverName,        0, "a1kw2k"
HKR, NDIS, MajorNdisVersion,     1, 04
HKR, NDIS, MinorNdisVersion,     1, 00

;*******************************************************************************
; Board Specific Driver parameters
;*******************************************************************************

[Altima.Params]
HKR, , RxPacketDescLowWaterMark,        0, "40"
HKR, , VlanEnable,                      0, "0"
HKR, , NumOfMapRegisters,               0, "32"
HKR, , TxPacketDescCnt,                 0, "200"
HKR, , RxStdDescCnt,                    0, "200"
HKR, , RxCoalescingTicks,               0, "360"
HKR, , TxCoalescingTicks,               0, "360"
HKR, , RxMaxCoalescedFrames,            0, "15"
HKR, , TxMaxCoalescedFrames,            0, "75"
HKR, , RxCoalescingTicksDuringInt,      0, "0"
HKR, , TxCoalescingTicksDuringInt,      0, "0"
HKR, , RxMaxCoalescedFramesDuringInt,   0, "0"
HKR, , TxMaxCoalescedFramesDuringInt,   0, "0"
HKR, , StatsCoalescingTicks,            0, "1000000"
HKR, , TxBufferSize,                    0, "0"
HKR, , RxJumboDescCnt,                  0, "0"
HKR, , RxMtu,                           0, "1500"
HKR, , DisableAutoNeg,                  0, "1"
HKR, , ResetPhyOnInit,                  0, "1"

HKR, Ndi\Params\RequestedMediaType,      ParamDesc, , "Speed & Duplex"
HKR, Ndi\Params\RequestedMediaType,      default,   , "0"
HKR, Ndi\Params\RequestedMediaType,      type,      , "enum"
HKR, Ndi\Params\RequestedMediaType\enum, 0,  , "Auto"
HKR, Ndi\Params\RequestedMediaType\enum, 3,  , "10 Mb Half"
HKR, Ndi\Params\RequestedMediaType\enum, 4,  , "10 Mb Full"
HKR, Ndi\Params\RequestedMediaType\enum, 5,  , "100 Mb Half"
HKR, Ndi\Params\RequestedMediaType\enum, 6,  , "100 Mb Full"
;HKR, Ndi\Params\RequestedMediaType\enum, 7,  , "1 Gb Half"
;HKR, Ndi\Params\RequestedMediaType\enum, 8,  , "1 Gb Full"

HKR, Ndi\Params\TaskOffloadCap,      ParamDesc, , "Checksum Offload"
HKR, Ndi\Params\TaskOffloadCap,      default,   , "21"
HKR, Ndi\Params\TaskOffloadCap,      type,      , "enum"
HKR, Ndi\Params\TaskOffloadCap\enum, 0,  , "None"
HKR, Ndi\Params\TaskOffloadCap\enum, 42, , "Rx TCP/IP Checksum"
HKR, Ndi\Params\TaskOffloadCap\enum, 21, , "Tx TCP/IP Checksum"
HKR, Ndi\Params\TaskOffloadCap\enum, 63, , "Tx/Rx TCP/IP Checksum"

HKR, Ndi\Params\WakeUpModeCap,       ParamDesc, , "Wake Up Capabilities"
HKR, Ndi\Params\WakeUpModeCap,       default,   , "3"
HKR, Ndi\Params\WakeUpModeCap,       type,      , "enum"
HKR, Ndi\Params\WakeUpModeCap\enum,  0,  , "None"
HKR, Ndi\Params\WakeUpModeCap\enum,  1,  , "Magic Packet"
HKR, Ndi\Params\WakeUpModeCap\enum,  2,  , "Wake Up Frame"
HKR, Ndi\Params\WakeUpModeCap\enum,  3,  , "Both"

HKR, Ndi\Params\Enable8021p,      ParamDesc, , "802.1p QOS"
HKR, Ndi\Params\Enable8021p,      default,   , "0"
HKR, Ndi\Params\Enable8021p,      type,      , "enum"
HKR, Ndi\Params\Enable8021p\enum, 0,  , "Disable"
HKR, Ndi\Params\Enable8021p\enum, 1,  , "Enable"

[Altima.Fibre.Params]
HKR, , EnableTbi,                  0, "1"

HKR, , RxPacketDescLowWaterMark,        0, "40"
HKR, , VlanEnable,                      0, "0"
HKR, , NumOfMapRegisters,               0, "32"
HKR, , TxPacketDescCnt,                 0, "200"
HKR, , RxStdDescCnt,                    0, "200"
HKR, , RxCoalescingTicks,               0, "360"
HKR, , TxCoalescingTicks,               0, "360"
HKR, , RxMaxCoalescedFrames,            0, "15"
HKR, , TxMaxCoalescedFrames,            0, "75"
HKR, , RxCoalescingTicksDuringInt,      0, "0"
HKR, , TxCoalescingTicksDuringInt,      0, "0"
HKR, , RxMaxCoalescedFramesDuringInt,   0, "0"
HKR, , TxMaxCoalescedFramesDuringInt,   0, "0"
HKR, , StatsCoalescingTicks,            0, "1000000"
HKR, , TxBufferSize,                    0, "0"
HKR, , RxJumboDescCnt,                  0, "0"
HKR, , RxMtu,                           0, "1500"
HKR, , DisableAutoNeg,                  0, "1"
HKR, , ResetPhyOnInit,                  0, "1"

HKR, Ndi\Params\RequestedMediaType,      ParamDesc, , "Speed & Duplex"
HKR, Ndi\Params\RequestedMediaType,      default,   , "0"
HKR, Ndi\Params\RequestedMediaType,      type,      , "enum"
HKR, Ndi\Params\RequestedMediaType\enum, 0,  , "Auto"
HKR, Ndi\Params\RequestedMediaType\enum, 8,  , "1 Gb Full"

HKR, Ndi\Params\TaskOffloadCap,      ParamDesc, , "Checksum Offload"
HKR, Ndi\Params\TaskOffloadCap,      default,   , "21"
HKR, Ndi\Params\TaskOffloadCap,      type,      , "enum"
HKR, Ndi\Params\TaskOffloadCap\enum, 0,  , "None"
HKR, Ndi\Params\TaskOffloadCap\enum, 42, , "Rx TCP/IP Checksum"
HKR, Ndi\Params\TaskOffloadCap\enum, 21, , "Tx TCP/IP Checksum"
HKR, Ndi\Params\TaskOffloadCap\enum, 63, , "Tx/Rx TCP/IP Checksum"

HKR, Ndi\Params\Enable8021p,      ParamDesc, , "802.1p QOS"
HKR, Ndi\Params\Enable8021p,      default,   , "0"
HKR, Ndi\Params\Enable8021p,      type,      , "enum"
HKR, Ndi\Params\Enable8021p\enum, 0,  , "Disable"
HKR, Ndi\Params\Enable8021p\enum, 1,  , "Enable"

;*******************************************************************************
; Destination directories
;*******************************************************************************

[DestinationDirs]
DefaultDestDir  = 11
CopyFile.Altima.Sys = 12
CopyFile.W9xSys = 11

[SourceDisksNames]
1 = %DISK_DESC%,,,

[SourceDisksFiles]
a1kw2k.sys = 1

[CopyFile.Altima.Sys]
a1kw2k.sys,,,

[CopyFile.W9xSys]
a1kw2k.sys,,,


;*******************************************************************************
; Localizable strings
;*******************************************************************************

[Strings]
ALTM  = "Altima"

ALTIMA1000C = "Altima 1000 Gigabit Ethernet  (Copper)"

ALTIMA1001C = "Altima 1001 Gigabit Ethernet  (IntegratedCopper)"

ALTIMA1002C = "Altima 1002 Gigabit Ethernet  (IntegratedCopper)"

ALTIMA1003C = "Altima 1003 Gigabit Ethernet  (IntegratedCopper)"

ALTIMA1000F = "Altima 1000 Gigabit Ethernet  (Fibre)"

DISK_DESC = "Altima Driver Diskette"


; Driver Information Entries
DriverMfgr="Altima"                                         ; IHV name
DriverVersionID="3.12"                                   ; The IHV driver version
BaseDriverFileVersion="3.12"                           ; version of key file
BaseDriverFileName="a1kw2k.sys"                ; Key file for version

; These items will be set by IHV and updated by OEM
DriverOEM="Altima"                                      ; name of the OEM
DriverFamily="NIC"                                    ; device family (NIC, Storage, Video...)
DriverProduct="AC100X"                            ; Specific Name of device (chipset, for example)
DriverDescription="Altima Gigabit Ethernet"  ; Description of device (product name, OS or system supported)
DriverOEMVersion="A00"                                ; OEM-specified version


