[DLKFET]
Type = NDIS
Title = "Legend/D-Link DFE-530TX PCI Fast Ethernet Adapter"
Version = 2.72
Drivername = DLKFET$
Xports = NETBEUI LANDD

[FILE]
Name = DLKFET.DOS

; Parameter start

[NETWORKADDRESS]
tag = NETWORKADDRESS
display = "Network adapter address"
type = Hexstring
Strlength = 12
optional = YES
editable = YES
help = "This parameter overrides the network address of the network
 adapter card.  The value of this parameter is a hexadecimal string of
 12 digits, as in 020001020304.  The address
 must be unique among all other network adapter addresses on the
 network."

[SLOT]
tag = SLOT
display = "Slot Number"
type = decimal
range = 1 - 16
optional = YES
editable = YES
help = "This parameter specifies the slot number used for notifications."


[CONNECTIONTYPE]
tag = CONNECTIONTYPE
display = "Connection Type"
type = string
Strlength = 14
Set = AUTOSENSE, _10BASET, _10BASETFD, _100BASETX, _100BASETXFD
default = AUTOSENSE
optional = YES
editable = YES
help = "This parameter specifies the connector type configuration of
 the  network adapter card.  The specification of this parameter depends
 on the specific hardware configuration.  This parameter is used only
 for the Legend/D-Link DFE-530TX PCI adapter for Personal Computer AT workstations.
 The parameters are AUTOSENSE, _10BASET, _10BASETFD, _100BASETX,
 and _100BASETXFD."
