;; NET8185.INF
;;
;; Realtek RTL8185 PCI/Cardbus 802.11g 54M Wireless LAN Network Interface Cards.
;;
;; Copyright 1996-2004, Realtek Semiconductor Corporation
;;

[version]
Signature      = "$Chicago$"
Compatible     = 1
Class          = Net
ClassGUID      = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider       = %Realtek%                                 ;;
CatalogFile    = net8185.cat                               ;; for WHQL certified
;CatalogFile.NT = net8185n.cat
DriverVer      = 02/08/2006,5.105.0.1

[Manufacturer]
%Realtek%   = Realtek

[ControlFlags]
ExcludeFromSelect     = PCI\VEN_10EC&DEV_8185
ExcludeFromSelect     = PCI\VEN_10EC&DEV_8185&SUBSYS_818510EC  
ExcludeFromSelect     = PCI\VEN_10EC&DEV_8185&SUBSYS_616510E8                      

[Realtek]
%RTL8185.DeviceDesc%  = RTL8185.ndi, PCI\VEN_10EC&DEV_8185
%RTL8185.DeviceDesc%  = RTL8185.ndi, PCI\VEN_10EC&DEV_8185&SUBSYS_818510EC
%RTL8185.DeviceDesc%  = RTL8185.ndi, PCI\VEN_10EC&DEV_8185&SUBSYS_616518E8 

;;****************************************************************************
;; Windows 9x
;;****************************************************************************
[RTL8185.ndi]
DriverVer       = 02/08/2006,105
AddReg          = rtl8185.id.reg, RTL8185.common.reg, RTL8185.win.reg
CopyFiles       = RTL8185.CopyFiles98

;;****************************************************************************
;; NT 5.0
;;****************************************************************************
[RTL8185.ndi.NT]
AddReg          = RTL8185.common.reg, RTL8185.reg
Characteristics = 0x84
BusType         = 5
CopyFiles       = RTL8185.CopyFiles

[RTL8185.ndi.NT.Services]
AddService = rtl8185, 2, rtl8185.Service, RTL8185.EventLog

[RTL8185.CopyFiles]
rtl8185.sys,,,2

[RTL8185.CopyFiles98]
rtl8185.sys,,,2

;;----------------------------------------------------------------------------
;; RTL8185 Parameters
;;----------------------------------------------------------------------------
;;***************************************************************************
;; Windows 9x parameters
;;***************************************************************************
[rtl8185.id.reg]
HKR, Ndi,       DeviceID,       0,      "PCI\VEN_10EC&DEV_8185"

HKR, Ndi\Install,                       ,       0,      rtsnt.install
HKR, NDI\Params\NetworkAddress,         flag,   1,      30, 00, 00, 00

[RTL8185.win.reg]
;; key,subkey,valuname,type,value
HKR, ,  DriverDesc,     0,      "Realtek RTL8185 54M Wireless LAN Network Adapter"
HKR, ,  DevLoader,      0,      *ndis
HKR, ,  DeviceVxDs,     0,      rtl8185.sys
HKR, ,  EnumPropPages,  0,      netdi.dll,      EnumPropPages

;;params
HKR, ,  MediaType,      0,      1
HKR, ,  AdapterType,    0,      5
HKR, ,  BusType,        0,      5

;; NDIS Info
HKR, NDIS,              MajorNdisVersion,       1,      03
HKR, NDIS,              MinorNdisVersion,       1,      0a
HKR, NDIS,              LogDriverName,          0,      "RTL8185"

;; Interfaces
HKR, Ndi\Interfaces,    DefLower,               ,       "ethernet"
HKR, Ndi\Interfaces,    LowerRange,             ,       "ethernet"
HKR, Ndi\Interfaces,    DefUpper,               ,       "ndis3"
HKR, Ndi\Interfaces,    UpperRange,             ,       "ndis3"

;; Install sections
HKR, Ndi\Install,       ndis3,                  0,      "rtl185.ndis5"

;;****************************************************************************
;; RTL8185 common parameters
;;****************************************************************************
[RTL8185.common.reg]
HKR,defaults,AH_BcnIntv, 0, "1000"
HKR,Ndi\params\AH_BcnIntv, default, 0, "100"
HKR,Ndi\params\AH_BcnIntv, ParamDesc, 0, %AH_BCNINTV_STR%
HKR,Ndi\params\AH_BcnIntv, type, 0, "int"
HKR,Ndi\params\AH_BcnIntv, min, 0, "20"
HKR,Ndi\params\AH_BcnIntv, max, 0, "1000"
HKR,Ndi\params\AH_BcnIntv, step, 0, "1"

HKR,defaults,FragThresh, 0, "2432"
HKR,Ndi\params\FragThresh, default, 0, "2432"
HKR,Ndi\params\FragThresh, ParamDesc, 0, %FRAGTHRESH_STR%
HKR,Ndi\params\FragThresh, type, 0, "int"
HKR,Ndi\params\FragThresh, min, 0, "256"
HKR,Ndi\params\FragThresh, max, 0, "2432"
HKR,Ndi\params\FragThresh, step, 0, "1"

HKR,defaults,ShortRetryLimit, 0, "7"
HKR,Ndi\params\ShortRetryLimit, default, 0, "7"
HKR,Ndi\params\ShortRetryLimit, ParamDesc, 0, "Short Retry Limit"
HKR,Ndi\params\ShortRetryLimit, type, 0, "int"
HKR,Ndi\params\ShortRetryLimit, min, 0, "0"
HKR,Ndi\params\ShortRetryLimit, max, 0, "255"
HKR,Ndi\params\ShortRetryLimit, step, 0, "1"

HKR,defaults,LongRetryLimit, 0, "7"
HKR,Ndi\params\LongRetryLimit, default, 0, "7"
HKR,Ndi\params\LongRetryLimit, ParamDesc, 0, "Long Retry Limit"
HKR,Ndi\params\LongRetryLimit, type, 0, "int"
HKR,Ndi\params\LongRetryLimit, min, 0, "0"
HKR,Ndi\params\LongRetryLimit, max, 0, "255"
HKR,Ndi\params\LongRetryLimit, step, 0, "1"

HKR,defaults,MaxPktSize, 0, "2432"
HKR,Ndi\params\MaxPktSize, default, 0, "1514"
HKR,Ndi\params\MaxPktSize, ParamDesc, 0, "Maximum Packet Size"
HKR,Ndi\params\MaxPktSize, type, 0, "int"
HKR,Ndi\params\MaxPktSize, min, 0, "200"
HKR,Ndi\params\MaxPktSize, max, 0, "2432"
HKR,Ndi\params\MaxPktSize, step, 0, "1"


;;

;HKR,Ndi\Params\RateDependentAck, ParamDesc, 0, "Enable Rate Dependent Ack"
;HKR,Ndi\Params\RateDependentAck, Type,      0, "enum"
;HKR,Ndi\Params\RateDependentAck, Default,   0, "0"
;HKR,Ndi\Params\RateDependentAck\enum, "0",  0, "Disable"
;HKR,Ndi\Params\RateDependentAck\enum, "1",  0, "Enable"

HKR,Ndi\params\NetworkAddress,   ParamDesc, 0, %NetworkAddress%
HKR,Ndi\params\NetworkAddress,   type,      0, "edit"
HKR,Ndi\params\NetworkAddress,   default,   0, "000000000000"
HKR,Ndi\params\NetworkAddress,   LimitText, 0, "12"
HKR,Ndi\params\NetworkAddress,   UpperCase, 0, "1"
HKR,Ndi\params\NetworkAddress,   Optional,  0, "1"

;HKR,NDI\Params\TxMaxDMABurst,flag,1,30,00,00,00
;HKR,Ndi\params\TxMaxDMABurst,ParamDesc,0,"Transmit DMA burst size"
;HKR,Ndi\params\TxMaxDMABurst,type,0,enum
;HKR,Ndi\params\TxMaxDMABurst,default,0,6
;HKR,Ndi\params\TxMaxDMABurst\enum,0,0,"0:16 bytes"
;HKR,Ndi\params\TxMaxDMABurst\enum,1,0,"1:32 bytes"
;HKR,Ndi\params\TxMaxDMABurst\enum,2,0,"2:64 bytes"
;HKR,Ndi\params\TxMaxDMABurst\enum,3,0,"3:128 bytes"
;HKR,Ndi\params\TxMaxDMABurst\enum,4,0,"4:256 bytes"
;HKR,Ndi\params\TxMaxDMABurst\enum,5,0,"5:512 bytes"
;HKR,Ndi\params\TxMaxDMABurst\enum,6,0,"6:1024 bytes"
;HKR,Ndi\params\TxMaxDMABurst\enum,7,0,"7:2048 bytes"

;HKR,NDI\Params\RxMaxDMABurst,flag,1,30,00,00,00
;HKR,Ndi\params\RxMaxDMABurst,ParamDesc,0,"Receive DMA burst size"
;HKR,Ndi\params\RxMaxDMABurst,type,0,enum
;HKR,Ndi\params\RxMaxDMABurst,default,0,6
;HKR,Ndi\params\RxMaxDMABurst\enum,0,0,"0:16 bytes"
;HKR,Ndi\params\RxMaxDMABurst\enum,1,0,"1:32 bytes"
;HKR,Ndi\params\RxMaxDMABurst\enum,2,0,"2:64 bytes"
;HKR,Ndi\params\RxMaxDMABurst\enum,3,0,"3:128 bytes"
;HKR,Ndi\params\RxMaxDMABurst\enum,4,0,"4:256 bytes"
;HKR,Ndi\params\RxMaxDMABurst\enum,5,0,"5:512 bytes"
;HKR,Ndi\params\RxMaxDMABurst\enum,6,0,"6:1024 bytes"
;HKR,Ndi\params\RxMaxDMABurst\enum,7,0,"7:unlimitted"

;HKR,NDI\Params\EarlyRxThreshold,flag,1,30,00,00,00
;HKR,Ndi\params\EarlyRxThreshold,ParamDesc,0,"Receive FIFO threshold"
;HKR,Ndi\params\EarlyRxThreshold,type,0,enum
;HKR,Ndi\params\EarlyRxThreshold,default,0,2
;HKR,Ndi\params\EarlyRxThreshold\enum,0,0,"0:16 bytes"
;HKR,Ndi\params\EarlyRxThreshold\enum,1,0,"1:32 bytes"
;HKR,Ndi\params\EarlyRxThreshold\enum,2,0,"2:64 bytes"
;HKR,Ndi\params\EarlyRxThreshold\enum,3,0,"3:128 bytes"
;HKR,Ndi\params\EarlyRxThreshold\enum,4,0,"4:256 bytes"
;HKR,Ndi\params\EarlyRxThreshold\enum,5,0,"5:512 bytes"
;HKR,Ndi\params\EarlyRxThreshold\enum,6,0,"6:1024 bytes"
;HKR,Ndi\params\EarlyRxThreshold\enum,7,0,"7:Disabled"

HKR,defaults,Channel,0,"1"
HKR,Ndi\params\Channel,default,	0,"1"
HKR,Ndi\params\Channel,ParamDesc,,%CHANNEL_STR%
HKR,Ndi\params\Channel,type,		,"int"
HKR,Ndi\params\Channel,flag,		1,"30","00","00","00"
HKR,Ndi\params\Channel,min,			0,"1"
HKR,Ndi\params\Channel,max,			0,"161"
HKR,Ndi\params\Channel,step,		0,"1"

HKR,defaults,PowerSaveMode,0,"0"
HKR,Ndi\params\PowerSaveMode,default,0,"0"
HKR,NDI\params\PowerSaveMode,ParamDesc,,%POWER_SAVE_STR%
HKR,NDI\params\PowerSaveMode,type,,"enum"
HKR,NDI\params\PowerSaveMode,flag,1,"30","00","00","00"
HKR,NDI\params\PowerSaveMode\enum,0,,"None"
HKR,NDI\params\PowerSaveMode\enum,2,,"Min"
HKR,NDI\params\PowerSaveMode\enum,1,,"Max"
;HKR,NDI\params\PowerSaveMode,optional,0,"1"

HKR,Ndi\params\SSID,   	ParamDesc, 	0, 	%SSID_STR%
HKR,defaults,			SSID,		0,	"ANY"
HKR,Ndi\params\SSID,   	type,      	0, 	"edit"
HKR,Ndi\params\SSID,   	default,   	0, 	"ANY"
HKR,Ndi\params\SSID,   	LimitText, 	0, 	"32"
;HKR,Ndi\params\SSID,   	Optional,  	0, 	"1"

HKR,Ndi\Params\ChannelPlan, ParamDesc, 0, "Channel Plan"
HKR,Ndi\Params\ChannelPlan, Type, 0, "enum"
HKR,Ndi\Params\ChannelPlan, Default, 0, "15"
HKR,Ndi\Params\ChannelPlan\enum, "0", 0, "FCC"
HKR,Ndi\Params\ChannelPlan\enum, "1", 0, "IC"
HKR,Ndi\Params\ChannelPlan\enum, "2", 0, "ETSI"
HKR,Ndi\Params\ChannelPlan\enum, "3", 0, "Spain"
HKR,Ndi\Params\ChannelPlan\enum, "4", 0, "France"
HKR,Ndi\Params\ChannelPlan\enum, "5", 0, "MKK"
HKR,Ndi\Params\ChannelPlan\enum, "6", 0, "MKK1"
HKR,Ndi\Params\ChannelPlan\enum, "7", 0, "Israel"
HKR,Ndi\Params\ChannelPlan\enum, "8", 0, "TELEC"
HKR,Ndi\Params\ChannelPlan\enum, "15", 0, "DOMAIN_FROM_EEPROM"

HKR,defaults,RSSIRoamingWeakSignalThreshold, 0, "100"
HKR,Ndi\params\RSSIRoamingWeakSignalThreshold, default, 0, "50"
HKR,Ndi\params\RSSIRoamingWeakSignalThreshold, ParamDesc, 0, "Roaming Weak Signal Threshold"
HKR,Ndi\params\RSSIRoamingWeakSignalThreshold, type, 0, "int"
HKR,Ndi\params\RSSIRoamingWeakSignalThreshold, min, 0, "0"
HKR,Ndi\params\RSSIRoamingWeakSignalThreshold, max, 0, "100"
HKR,Ndi\params\RSSIRoamingWeakSignalThreshold, step, 0, "1"

HKR,defaults,RSSIRoamingHeavyTrafficThreshold, 0, "100"
HKR,Ndi\params\RSSIRoamingHeavyTrafficThreshold, default, 0, "90"
HKR,Ndi\params\RSSIRoamingHeavyTrafficThreshold, ParamDesc, 0, "Roaming Heavy Traffic Threshold"
HKR,Ndi\params\RSSIRoamingHeavyTrafficThreshold, type, 0, "int"
HKR,Ndi\params\RSSIRoamingHeavyTrafficThreshold, min, 0, "0"
HKR,Ndi\params\RSSIRoamingHeavyTrafficThreshold, max, 0, "100"
HKR,Ndi\params\RSSIRoamingHeavyTrafficThreshold, step, 0, "1"

HKR,defaults,NetworkType,0,"1"
HKR,Ndi\params\NetworkType,default,0,"1"
HKR,NDI\params\NetworkType,ParamDesc,,%NETWORK_TYPE_STR%
HKR,NDI\params\NetworkType,type,,"enum"
HKR,NDI\params\NetworkType,flag,1,"30","00","00","00"
HKR,NDI\params\NetworkType\enum,0,,"Ad Hoc"
HKR,NDI\params\NetworkType\enum,1,,"Infrastructure"
HKR,NDI\params\NetworkType\enum,2,,"Auto select"
;HKR,NDI\params\NetworkType,optional,0,"1"

HKR,Ndi\Params\bRateAdaptive, ParamDesc, 0, "Rate Adaptive"
HKR,Ndi\Params\bRateAdaptive, Type, 0, "enum"
HKR,Ndi\Params\bRateAdaptive, Default, 0, "1"
HKR,Ndi\Params\bRateAdaptive\enum, "0", 0, "Disable"
HKR,Ndi\Params\bRateAdaptive\enum, "1", 0, "Enable"

HKR,,DefaultKeyID,,"0"
HKR,,DefaultKey0,,""
HKR,,DefaultKey1,,""
HKR,,DefaultKey2,,""
HKR,,DefaultKey3,,""

HKR,Ndi\Params\ConnectedOnIBSS, ParamDesc, 0, "IBSS Default Link State"
HKR,Ndi\Params\ConnectedOnIBSS, Type,      0, "enum"
HKR,Ndi\Params\ConnectedOnIBSS, Default,   0, "0"
HKR,Ndi\Params\ConnectedOnIBSS\enum, "0",  0, "Disable"
HKR,Ndi\Params\ConnectedOnIBSS\enum, "1",  0, "Enable"
;;****************************************************************************
;; NT 5.0 parameters
;;****************************************************************************
[RTL8185.reg]
HKR, Ndi\Interfaces,            UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces,            LowerRange, 0, "ethernet"
HKR, Ndi,                       Service,    0, "RTL8185"

[rtl8185.Service]
DisplayName     = %RTL8185.Service.DispName%
ServiceType     = 1                             ; %SERVICE_KERNEL_DRIVER%
StartType       = 3                             ; %SERVICE_DEMAND_START%
ErrorControl    = 1                             ; %SERVICE_ERROR_NORMAL%
ServiceBinary   = %12%\rtl8185.sys
LoadOrderGroup  = NDIS

[RTL8185.EventLog]
Addreg = RTL8185.AddEventLog.reg

[RTL8185.AddEventLog.reg]
HKR,    ,   EventMessageFile,   0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR,    ,   TypesSupported,     0x00010001, 7

;;****************************************************************************
;; Destination Directory
;;****************************************************************************
[DestinationDirs]
RTL8185.CopyFiles           = 12
RTL8185.CopyFiles98         = 11
DefaultDestDir              = 11        ; LDID_SYS

;;****************************************************************************
;; Source Files
;;****************************************************************************
[SourceDisksNames]
1=%DISKNAME%,,,

[SourceDisksFiles]
rtl8185.sys  = 1
;netr8185.inf  = 1
;netr8185.cat  = 1
;netr8185n.cat  = 1

;;****************************************************************************
;; Strings
;;****************************************************************************
[Strings]
Realtek                   = "Realtek"

;;Source disk name
DISKNAME = " Realtek RTL8185 54M Wireless LAN Network Adapter Driver Disk "

NetworkAddress =		"Network Address"
ADHOC_DEMO_STR = 		"Adhoc Demo Mode"
SHORT_PREAM_STR =		"Preamble Mode"
AH_BCNINTV_STR = 		"Beacon Interval"
AH_ATIMINTV_STR =		"Atim Window"
RTSTHRESH_STR =			"RTS Threshold"
FRAGTHRESH_STR =		"Fragmentation Threshold"
AUTHENT_TYPE_STR =		"Authentication Algorithm"
LISTENINTERVAL_STR =	"Listen Interval"
CHANNEL_STR	 =			"Channel"
DATA_RATE_STR =			"Data Rate"
POWER_SAVE_STR 	=		"Power Save Mode"
SSID_STR =				"SSID"
NETWORK_TYPE_STR =		"Network Type"
RTL8185.DeviceDesc =	"Realtek RTL8185 54M Wireless LAN Network Adapter"
RTL8185.Service.DispName =	"Realtek RTL8185 54M Wireless LAN Network Adapter Driver"
;
