
        Legend/D-Link DFE-530TX PCI Fast Ethernet Adapter Installation
                        for Windows NT V3.51


 Getting Started
 ---------------

   1. The Windows NT CD/disks are need to complete this installation

        - From the "Main" window, select Control Panel

        - In the Control Panel, select Network Icon

        - In the Network Setup, select Add Adapter

   2. Windows NT will display a list of all available drivers.

        - Select "OTHERS" for third-party adapters not included in the
          list.

   3. The program prompts for the directory containing the Ethernet drivers.

          Insert the driver diskette in Drive A, and then type
          the following:

          A:\

        - Windows NT will attempt to locate the OEMSETNT.INF file in the
          specified path. If it exists there, Windows NT will then copy
          the appropriate drivers to the Windows NT system.

        - The drivers are now properly installed. It also will pop up the
          configuration window, you can assign the "Connection Type" here
          The installation procedure will then proceed to the next steps.
          Please refer to your Windows NT installation guide for information
          on these steps.

        - After the initial installation, the drivers will be permanently
          installed to the Windows NT system.  Subsequent accesses to the
          network driver list will include these drivers as options.


        Driver keywords:
        ----------------

          Open "Main" -> "Control Pannel" -> "Network" ->
          Select "Legend/D-Link DFE-530TX ..." -> "Configure"

          Then you can choose "Connection Type"

           Auto-Negotiation     : The driver will auto-detect the media that
                                  is connecting to the adapter. (default)
           100BaseTX Half_duplex: The driver will force the media to
                                  100BaseTx half duplex mode.
           100BaseTX Full_duplex: The driver will force the media to
                                  100BaseTx full duplex mode.
           10BaseT Half_duplex  : The driver will force the media to
                                  10BaseT half duplex mode.
           10BaseT Full_duplex  : The driver will force the media to
                                  10BaseT full duplex mode.


           Choose the appropriate setting as needed.


