# Script to start "input" on the device, which has a very rudimentary
# shell.
#
export ANDROID_DATA=/data/local/tmp
export CLASSPATH=/data/local/tmp/bdim.jar
exec app_process /data/local/tmp com.baidu.carlife.touch.CarlifeInput $*

